**ANNEX 3 – BILL OF QUANTITIES**

|  |  |
| --- | --- |
| REF | GENERAL REMARK |
| QUOTED RATES ARE TO TAKE INTO CONSIDERATION ALL DOUBLE HANDLING OF MATERIAL AS WELL AS COMPLIANCE WITH RELEVANT STANDARDS, LEGAL NOTICES AND HEALTH AND SAFETY PROCEDURES. THE CONTRACTOR IS RESPONSIBLE FOR ANY DAMAGE CAUSED TO EXISTING STRUCTURES AND HAS TO MAKE GOOD AT HIS OWN EXPENSE. NO EXTRA REMUNERATION IS FORESEEN | |

**Section 1**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **2** | **Pellet production line** | |  | |  |
| No. | Description | Unit | Quantity | Offered Unit price in $ | Offered Total price in $ (including VAT, if applicable ) |
| 1 | Mill for reed:   * Massive iron construction with possibility to mount on the floor * Electric engine powered (min 4 Kv) * Rotor with crushers at least 5 mm wide * Cyclone installed * Capacity: min 100 kg/h * Output chips range compatible with item no 2 | piece | 1 |  |  |
|  | Pelleting machine:   * Massive iron construction with possibility to mount on the floor * Ring matrix minimum θ 250 mm * Minimum two rollers * Feeding container * Control electro panel * Fully compatible with item no 1 | piece | 1 |  |  |
| Cooler of products from pelleting machine:   * Vibro-screen * Centrifugal fan * Fully compatible with item no 2 | piece | 1 |  |  |
|  | Transport line:   * Conveyer belt type * Width min 0.3 m, length min 4 m * Fully compatible with item no 3 | piece | 1 |  |  |
|  | Storage container for final product:   * Massive iron construction with possibility to mount on the floor * Minimum storage capacity: 1 m3 * Coinvent outlet for product evacuation * -Fully compatible with item no 4 | piece | 1 |  |  |
|  | Delivery of all goods to the Vranjina, Montenegro | fee | 1 |  |  |
|  |  | TOTAL SECTION 2: | | | $ |

**Section 2**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Machines forwood chopping** | |  | |  |
| No. | Description | Unit | Quantity | Offered Unit price in $ | Offered Total price in $ (including VAT) |
| 1 | Chopper:  - Petrol engine min 10 HP  - Minim crushing of the branches θ 6  - Blades, two pieces  - Large input area  - Large wheels  - Trailer hook  - Extension of ejection tube to be compatible with the tractor trailer: 4 tons case measurements 300X190X40+ (30) CM for collecting. | piece | 1 |  |  |
|  |  | TOTAL SECTION 3: | | | $ | |

Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ID: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_