# Annex 2

# Financial Offer Form

Quotation Ref: 33/2022/Zero Drop

Supplier’s Details:

|  |  |
| --- | --- |
| Type of Business (Company/Self-employed – Freelancer) |  |
| Company Name/supplier name: |  |
| Address: |  |
| Tel/ e-mail address: |  |
| VAT or Tax registration No: |  |
| Name of Legal Representative: |  |

Schedule of Rates:

Rates and Total price of each item is to be quoted in **Euros** **Including VAT and any other Tax or Fee** that should apply for any reason.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **A/A** | **Service / Task** | **Quantity** | **Unit Price (€)** | **VAT (€)** | **Total (€)** |
| **A. Supply and Installation** | | | | | |
| 1 | Supply and installation (on proper metal framework) of four (4) solar powered water producing panels (from the atmospheric moisture) at the roof of the concrete shed at the port.  Supply and Installation of one (1) water cooler to the four (4) panels.  Supply of a mobile device to be connected to screen and display the availability of water (including the HDMI cable).  The screen is out of the scope of the present supply.  Specific requirements:   * The piping from the solar powered water producing panels to the water cooler should be hidden (e.g. plastic piping channels) * The cables from the water cooler to the power source should be hidden (e.g. plastic piping channels). * The equipment should be delivered ready to operate.   The hiding of the piping and the cables behind is essential for those lines not to interfere with the make-over / decoration / preparation activities that will take place under the shed. | Lump sum |  |  |  |
| 2 | Supply and installation (on proper metal framework) of two (2) solar powered water producing panels (from the atmospheric moisture) at the roof of the municipality building.  Installation of one (1) existing water cooler to the four (4) panels on the roof of the municipality building.  Specific requirements:   * The piping from the solar powered water producing panels to the water cooler should be as discrete as possible or even hidden (e.g. plastic piping channels) * The equipment should be delivered ready to operate. | Lump sum |  |  |  |
|  | | | | | |
| **B. Drawings** | | | | | |
| 1 | Preliminary drawings on the installation array and the hydraulic connection. | 1 |  |  |  |
| 2 | Final drawings on the installation array and the hydraulic connection. | 1 |  |  |  |
|  | | | | | |
| **GRAND TOTAL (€)** | | | |  | |

The Participant I am representing (“We”) has examined, and accepts in full and in its entirety, the content of this quotation document (including subsequent Clarification Notes issued by the Contracting Authority). We hereby accept the contents thereto in their entirety, without reservation or restriction. We also understand that any disagreement, contradiction, alteration, deviation or omission shall lead to our offer not being considered any further. We offer to provide, in accordance with the terms of the tender document and the conditions and time limits laid down, without reservation or restriction, the requirements of this Request for Quotations (RfQ).

*\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*Signature Date*