# Annex 4

# Financial Offer Form

Quotation Ref: 12/2024/Resilient Thessaly

Supplier’s Details:

|  |  |
| --- | --- |
| Type of Business (Company/Self-employed – Freelancer) |  |
| Company Name/supplier name:  |  |
| Address: |  |
| Tel/ e-mail address:  |  |
| VAT or Tax registration No: |  |
| Name of Legal Representative:  |  |

The Participant is required to submit the Financial Offer in a separate password protected file.

The Financial Offer must provide a detailed cost breakdown. Provide separate figures for each functional grouping or category.

The Financial Offer is inclusive of all taxes, bank costs and any other expenses. The Financial Offer must cover all Participants’ obligations under the contract.

Prices shall be necessarily indicated in EURO, for comparison reasons, and any quoted rates are to take into consideration all double handling of material as well as compliance with relevant standards, legal notices and health and safety procedures.

Offers that do not indicate their prices in EURO or offers that indicate an equivalency between EURO and foreign currencies shall be rejected as inadmissible.

If the offered price is not clearly and expressly mentioned, the offer shall be rejected as inadmissible.

Any costs, expenses or services not expressly mentioned in the offer is regarded as being offered for free.

Offer prices shall remain unchanged throughout the offer validity period. In case an extension of offer validity period is requested, Participants shall not be entitled, when giving their consent for such an extension, to submit new or amended price lists.

The Contracting Authority shall reserve the right to request that Participants submit any information required for the documentation of the prices offered.

Schedule of Rates:

Rates and Total price of each item is to be quoted in **Euros** **Including VAT and any other Tax or Fee or Costs** that should apply for any reason.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **A/A** | **Service / Task** | **Unit** | **Quantity** | **Unit Price (€)** | **Total Price (€)** | **VAT (€)** | **Total (€)** |
| **A. Earthworks**  |
| **A1. Excavations** |
| **A1.1** | Excavation of underground network trenches in earthy or semi-rocky soil with lateral deposition of excavation products. Excavation depth up to 4.0 m | m3 | 228,00 |  |  |  |  |
| **A1.2** | Excavation of underground network trenches in earthy semi-rocky soil with the transport of excavation products. Excavation depth up to 4.0 m | m3 | 2.470,00 |  |  |  |  |
| **A1.3** | Excavation dealing with additional difficulties from passing mains | m | 285,00 |  |  |  |  |
| **A1.4** | Excavation to be executed under conditions of limited space | m3 | 100,00 |  |  |  |  |
|  |
| **A2. Clearings / Restorations** |
| **A2.1** | Demolition of unreinforced concrete structures | m3 | 27,00 |  |  |  |  |
| **A2.2** | Restoration of single-layer asphalt pavements | m2 | 775,00 |  |  |  |  |
| **A2.3** | Asphalt precoating | m2 | 205,00 |  |  |  |  |
| **A2.4** | 0.05 m thick compacted asphaltic traffic layer using common ashpalt | m2 | 205,00 |  |  |  |  |
| **A2.5** | Loading and unloading of excavation products | m3 | 110,00 |  |  |  |  |
|  |
| **A3. Embankments** |
| **A3.1** | Backfilling trenches with excavated products with special compaction requirements | m3 | 228,00 |  |  |  |  |
| **A3.2** | Backfilling of trenches with brittle quarry material, for a total backfill thickness of more than 50 cm | m3 | 1.120,00 |  |  |  |  |
| **A3.3** | Laying and formwork of pipes with quarry sand | m3 | 645,00 |  |  |  |  |
| **A3.4** | Sanitizing layers with brittle quarry material | m3 | 110,00 |  |  |  |  |
|  |
| **A4. Water Treatment** |
| **A4.1** | Diesel or electric pump sets from 2 to 5 HP | h | 60 |  |  |  |  |
|  |
| **A5. Support** |
| **A5.1** | Trench side supports with metal curtains | m2 | 1.156,00 |  |  |  |  |
|  |
| **Sub-Total Group A** |  |  |  |
|  |
| **B. Concrete Constructions, Sealing, Building Works** |
| **B1.** **Concrete Constructions** |
| **B1.1** | Production, transportation, placing, compaction and maintenance of concrete, For concrete constructions of class C16/20 | m3 | 25,00 |  |  |  |  |
| **B1.2** | Typical control shafts | pcs | 4,00 |  |  |  |  |
| **B1.3** | Steel structural mesh B500C for outside underground works | kg | 330,00 |  |  |  |  |
|  |
| **Sub-Total Group B** |  |  |  |
|  |
| **C. Networks, Metal Elements and Structures, Piping Network Devices** |
| **C1. Piping / Networks** |
| **C1.1** | Networks with pipes SN8, DN/ID 1200 mm | m | 340,00 |  |  |  |  |
| **C1.2** | Ductile iron covers | kg | 160,00 |  |  |  |  |
| **C1.3** | Pipeline connection to an existing well | pcs | 14,00 |  |  |  |  |
|  |
| **Sub-Total Group C** |  |  |  |
|  |
| **GRAND TOTAL** |  |  |  |

The Participant I am representing (“We”) has examined, and accepts in full and in its entirety, the content of this quotation document (including subsequent Clarification Notes issued by the Contracting Authority). We hereby accept the contents thereto in their entirety, without reservation or restriction. We also understand that any disagreement, contradiction, alteration, deviation or omission shall lead to our offer not being considered any further. We offer to provide, in accordance with the terms of the tender document and the conditions and time limits laid down, without reservation or restriction, the requirements of this Request for Quotations (RfQ).

*\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*Signature Date*