Annex 4: Financial Offer Form / Call for Offers 07/2022/ Matchmaker 2

The Participant is required to submit the Financial Offer in an separate password protected file

The Financial Offer must provide a detailed cost breakdown. Provide separate figures for each functional grouping or category.

The Financial Offer, is inclusive of all taxes, bank costs and any other expenses. The Financial Offer must cover all Participants’ obligations under the contract.

Prices shall be necessarily indicated in **EURO, for comparison reasons,** and any quoted rates are to take into consideration all double handling of material as well as compliance with relevant standards, legal notices and health and safety procedures.

Offers that do not indicate their prices in EURO or offers that indicate an equivalency between EURO and foreign currencies shall be rejected as inadmissible.

If the offered price is not clearly and expressly mentioned, the offer shall be rejected as inadmissible.

Any costs, expenses or services not expressly mentioned in the offer is regarded as being offered for free.

Offer prices shall remain unchanged throughout the offer validity period. In case an extension of offer validity period is requested, Participants shall not be entitled, when giving their consent for such an extension, to submit new or amended price lists.

The Contracting Authority shall reserve the right to request that Participants submit any information required for the documentation of the prices offered.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item** | **Description** | **Unit** | **Quantity** | **Price per Item (€)** | **VAT** | **Total (€)** |
|  |  |  | **A. Drawings** |
| 01 | Preliminary drawings (constructed wetland, solar panels) – mechanical and electrical | Lump sum | 1 |  |  |  |
| 02 | As Built drawings (constructed wetland, solar panels) – mechanical and electrical | Lump sum | 1 |  |  |  |
|  |  |  |  |
|  |  |  | **B. Works** |
| 01 | Site cleaning for the constructed wetland and the solar panels (in each farm). | Lump sum | 3 |  |  |  |
| 02 | Construction of fully operational constructed wetland of 160 m2 (as specified), including irrigation tank of 2 m3, recirculation pump (7m3/d), inlet pump, filtering media, lining, inlet / outlet piping, etc. | Lump sum | 3 |  |  |  |
| 03 | Installation of timed irrigation pumps for the irrigation of the additional trees which will be installed (including el. Board). | Pcs | 6 (3 duty + 3 standby) |  |  |  |
| 04 | Connection of the irrigation tank with new pumps (one in each farm). | Lump sum | 3 |  |  |  |
| 05 | Construction of a fully operational solar power system of 6 kWp (as specified) | Lump sum | 1 |  |  |  |
| 06 | Construction of a fully operational solar power system of 7 kWp (as specified) | Lump sum | 1 |  |  |  |
| 07 | Construction of a fully operational solar power system of 24 kWp (as specified) | Lump sum | 1 |  |  |  |
| 08 | Connection of the solar power systems to the grid. | Lump sum | 3 |  |  |  |
| 09 | Fencing around the constructed wetlands to avoid accidents after the completion of the works (one in each farm), including gate of 4m width. | Lump sum | 3 |  |  |  |
| 10 | Fencing around the solar power systems to avoid accidents after the completion of the works (one in each farm) – including gate of 4m width. | Lump sum | 3 |  |  |  |
| 11 | Supply and plantation of trees in the farms (per farm/total) \*Mango AvocadoMoringaLemon or OrangePermanganate\* The selection of the trees to be planted will be made after consulting with the farm owners and the GWP-Med representative  | Pcs | 125/375 |  |  |  |
| 12 | Construction of irrigation network of 3 donums for the new trees (one in each farm) | Lump sum | 3 |  |  |  |
| 13 | Rehabilitation of the area of construction (remove materials that are not needed in the area for the operation of the interventions) | Lump sum | 3 |  |  |  |
|  |  |  |  |
|  |  |  | **C. Additional Equipment** |
| 01 | Portable Moisture Meter | Pcs | 3 |  |  |  |
|  |  |  |  |
|  |  |  | **D. Licensees, Fees, Certificates** |
| 01 | The Successful Contractor is responsible for all fees required for obtaining all approvals and permits required for the Assignment including the GIS fees. | Lump sum | a.a. |  |  |  |
| **Grand Total** |  |

The Participant I am representing (“We”) has examined, and accept in full and in its entirety, the content of this quotation document (including subsequent Clarification Notes issued by the Contracting Authority). We hereby accept the contents thereto in their entirety, without reservation or restriction. We also understand that any disagreement, contradiction, alteration, deviation or omission shall lead to our offer not being considered any further. We offer to provide, in accordance with the terms of the tender document and the conditions and time limits laid down, without reservation or restriction, the requirements of this Call For Offers

*\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*Signature Date*