**ANNEX 2**

**TECHNICAL SPECIFICATIONS AND MAX AVAILABLE PRICE PER ITEM**

**Section 1**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Pellet production line** | | **Max AVAILABLE Total** | | **$ 18,100.00** |
| No. | Description | Unit | Quantity | MaxUnit price | MaxTotal price |
| 1 | Mill for reed:   * Massive iron construction with possibility to mount on the floor * Electric engine powered (min 4 Kv) * Rotor with crushers at least 5 mm wide * Cyclone installed * Capacity: min 100 kg/h * Output chips range compatible with item no 2 | piece | 1 | 3,750 USD | 3,750 USD |
| 2 | Pelleting machine:   * Massive iron construction with possibility to mount on the floor * Ring matrix minimum θ 250 mm * Minimum two rollers * Feeding container * Control electro panel * Fully compatible with item no 1 | piece | 1 | 8,550 USD | 8,550 USD |
| 3 | Cooler of products from pelleting machine:   * Vibro-screen * Centrifugal fan * Fully compatible with item no 2 | piece | 1 | 3,100 USD | 3,100 USD |
| 4 | Transport line:   * Conveyer belt type * Width min 0.3 m, length min 4 m * Fully compatible with item no 3 | piece | 1 | 1,800 USD | 1,800 USD |
| 5 | Storage container for final product:   * Massive iron construction with possibility to mount on the floor * Minimum storage capacity: 1 m3 * Coinvent outlet for product evacuation * Fully compatible with item no 4 | piece | 1 | 900 USD | 900 USD |

**Section 2**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Machine for wood chopping** | | **Max AVAILABLE Total** | | **$ 5,000.00** |
| No. | Description | Unit | Quantity | MaxUnit price | MaxTotal price |
| 1 | Chopper:  - Petrol engine min 10 HP  - Minim crushing of the branches θ 6  - Blades, two pieces  - Large input area  - Large wheels  - Trailer hook  - Extension of ejection tube to be compatible with the tractor trailer: 4 tons case measurements 300X190X40+ (30) CM for collecting. | piece | 1 | 5,000 USD | 5,000 USD |