**ANNEX 2**

**TECHNICAL SPECIFICATIONS AND MAX AVAILABLE PRICE PER ITEM**

**Section 1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Pellet production line** | **Max AVAILABLE Total**  | **$ 18,100.00**  |
| No.  | Description  | Unit  | Quantity  | MaxUnit price  | MaxTotal price  |
| 1  | Mill for reed:* Massive iron construction with possibility to mount on the floor
* Electric engine powered (min 4 Kv)
* Rotor with crushers at least 5 mm wide
* Cyclone installed
* Capacity: min 100 kg/h
* Output chips range compatible with item no 2
 | piece  | 1  | 3,750 USD | 3,750 USD |
| 2 | Pelleting machine:* Massive iron construction with possibility to mount on the floor
* Ring matrix minimum θ 250 mm
* Minimum two rollers
* Feeding container
* Control electro panel
* Fully compatible with item no 1
 | piece | 1 | 8,550 USD | 8,550 USD |
| 3 | Cooler of products from pelleting machine:* Vibro-screen
* Centrifugal fan
* Fully compatible with item no 2
 | piece | 1 | 3,100 USD | 3,100 USD |
| 4 | Transport line:* Conveyer belt type
* Width min 0.3 m, length min 4 m
* Fully compatible with item no 3
 | piece | 1 | 1,800 USD | 1,800 USD |
| 5 | Storage container for final product:* Massive iron construction with possibility to mount on the floor
* Minimum storage capacity: 1 m3
* Coinvent outlet for product evacuation
* Fully compatible with item no 4
 | piece | 1 | 900 USD | 900 USD |

**Section 2**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Machine for wood chopping**  | **Max AVAILABLE Total** | **$ 5,000.00**  |
| No.  | Description  | Unit  | Quantity  | MaxUnit price  | MaxTotal price  |
| 1  | Chopper: - Petrol engine min 10 HP - Minim crushing of the branches θ 6- Blades, two pieces - Large input area - Large wheels - Trailer hook - Extension of ejection tube to be compatible with the tractor trailer: 4 tons case measurements 300X190X40+ (30) CM for collecting. | piece  | 1  | 5,000 USD | 5,000 USD |